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Text Elements for Specifications
STAUFF ACT Clamp Bodies
Small bore tubing assemblies up to 42 mm / 1 1/2 inch outside diameter shall be supported by block-type pipe clamps. The clamps shall be dimensionally in accordance with the DIN 3015 standard and suitable for single, twin and multi-level tube installations. Block-type clamps shall also be suitable for tray, plate or channel mounting.
To prevent the accumulation of seawater and the formation of crevice corrosion, the clamp body shall have drainage capabilities between the body and tube by utilizing integrated anti-corrosion strips that form part of the original clamp body design, thus allowing the free flow of seawater. Clamp bodies shall at no point be in direct contact with the tube material being supported.
STAUFF ACT Mounting Hardware
Evidence must be given that stainless steel 316 support accessories used for the fixing of clamps to structure have been subject to a cleaning process or are manufactured in a clean environment thereby removing foreign particles. It is required that evidence be provided at the time of acceptance of improved performance as a direct result of the cleaning process.
In order to ensure good performance for asset integrity, the selected product shall demonstrate its suitability by meeting and/or exceeding the minimum test standards in accordance with test standard 1104000110.
July 2021	Page 1 of 1	www.stauff.com/act 
image1.jpg
L~ ®
a2 STAUFF





